Skirt Line Count
====
This setting configures the number of contours to draw around the print, for the skirt.

One of the purposes of the skirt is to prime the nozzle, to get the material flowing properly. With very small models, a single line is not enough, so you can configure the skirt to be drawn with multiple lines.

Using the [Skirt/Brim Minimum Length](skirt_brim_minimal_length.md) setting is more reliable than using this setting to ensure a minimum amount of primed material. This setting is only somewhat easier to understand.